(module DSUB-15-HD_Female_Horizontal_P2.29x2.54mm (layer F.Cu) (tedit 5EC0FB33)
  (descr "15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
  (tags "15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
  (fp_text reference J1 (at -3.683 -5.1562) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value DB15_Female_HighDensity_MountingHoles (at -4.315 20.21) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at -4.315 15.71) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 11.65 -3.9) (end -20.25 -3.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11.65 19.25) (end 11.65 -3.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start -20.25 19.25) (end 11.65 19.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -20.25 -3.9) (end -20.25 19.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 -2.101325) (end -0.25 -2.534338) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.25 -2.534338) (end 0 -2.101325) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.25 -2.534338) (end 0.25 -2.534338) (layer F.SilkS) (width 0.12))
  (fp_line (start 11.17 -3.44) (end 11.17 12.25) (layer F.SilkS) (width 0.12))
  (fp_line (start -19.8 -3.44) (end 11.17 -3.44) (layer F.SilkS) (width 0.12))
  (fp_line (start -19.8 12.25) (end -19.8 -3.44) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.785 12.31) (end 9.785 1.42) (layer F.Fab) (width 0.1))
  (fp_line (start 6.585 12.31) (end 6.585 1.42) (layer F.Fab) (width 0.1))
  (fp_line (start -15.215 12.31) (end -15.215 1.42) (layer F.Fab) (width 0.1))
  (fp_line (start -18.415 12.31) (end -18.415 1.42) (layer F.Fab) (width 0.1))
  (fp_line (start 10.685 12.71) (end 5.685 12.71) (layer F.Fab) (width 0.1))
  (fp_line (start 10.685 17.71) (end 10.685 12.71) (layer F.Fab) (width 0.1))
  (fp_line (start 5.685 17.71) (end 10.685 17.71) (layer F.Fab) (width 0.1))
  (fp_line (start 5.685 12.71) (end 5.685 17.71) (layer F.Fab) (width 0.1))
  (fp_line (start -14.315 12.71) (end -19.315 12.71) (layer F.Fab) (width 0.1))
  (fp_line (start -14.315 17.71) (end -14.315 12.71) (layer F.Fab) (width 0.1))
  (fp_line (start -19.315 17.71) (end -14.315 17.71) (layer F.Fab) (width 0.1))
  (fp_line (start -19.315 12.71) (end -19.315 17.71) (layer F.Fab) (width 0.1))
  (fp_line (start 3.835 12.71) (end -12.465 12.71) (layer F.Fab) (width 0.1))
  (fp_line (start 3.835 18.71) (end 3.835 12.71) (layer F.Fab) (width 0.1))
  (fp_line (start -12.465 18.71) (end 3.835 18.71) (layer F.Fab) (width 0.1))
  (fp_line (start -12.465 12.71) (end -12.465 18.71) (layer F.Fab) (width 0.1))
  (fp_line (start 11.11 12.31) (end -19.74 12.31) (layer F.Fab) (width 0.1))
  (fp_line (start 11.11 12.71) (end 11.11 12.31) (layer F.Fab) (width 0.1))
  (fp_line (start -19.74 12.71) (end 11.11 12.71) (layer F.Fab) (width 0.1))
  (fp_line (start -19.74 12.31) (end -19.74 12.71) (layer F.Fab) (width 0.1))
  (fp_line (start 11.11 -3.38) (end -19.74 -3.38) (layer F.Fab) (width 0.1))
  (fp_line (start 11.11 12.31) (end 11.11 -3.38) (layer F.Fab) (width 0.1))
  (fp_line (start -19.74 12.31) (end 11.11 12.31) (layer F.Fab) (width 0.1))
  (fp_line (start -19.74 -3.38) (end -19.74 12.31) (layer F.Fab) (width 0.1))
  (fp_arc (start 8.185 1.42) (end 6.585 1.42) (angle 180) (layer F.Fab) (width 0.1))
  (fp_arc (start -16.815 1.42) (end -18.415 1.42) (angle 180) (layer F.Fab) (width 0.1))
  (pad 0 thru_hole circle (at 8.185 1.42) (size 4 4) (drill 3.05) (layers *.Cu *.Mask))
  (pad 0 thru_hole circle (at -16.815 1.42) (size 4 4) (drill 3.05) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at -9.16 3.96) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at -6.87 3.96) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at -4.58 3.96) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at -2.29 3.96) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 0 3.96) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at -8.015 1.42) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at -5.725 1.42) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at -3.435 1.42) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at -1.145 1.42) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 1.145 1.42) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -9.16 -1.12) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -6.87 -1.12) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -4.58 -1.12) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -2.29 -1.12) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 -1.12) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-15-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
